SIMISA@@@@@@@@@@JINX0D0t______

Wagon      ( PKP_TKt48-113_m
   comment ( *wersja 2.0 OR polish depot 05.07.2022* )
Type       ( Engine )
WagonShape ( PKP_TKt48-113.s )

ORTSFreightAnims
(
MSTSFreightAnimEnabled ( 0 )
FreightAnimStatic
(
SubType ( Default )
Shape   ( ../common.fa/zaloga.s )
Offset  ( 0.0 0.29 0.00 )
)
FreightAnimStatic
(
SubType ( Default )
Shape   ( cien_TKt48.s )
Offset  ( 0.0 0.0 0.0 )
)
)
Include		("../common.inc/Parowozy/Tkt48/Size_Tkt48_v2.inc")
Sound     ( "..//..//common.snd//dampf_BR64//BR64Eng.sms" )
Include		("../common.inc/Parowozy/Tkt48/Coupler_Tkt48.inc")
Include		("../common.inc/Parowozy/Tkt48/Brakes_Tkt48.inc")
Include		("../common.inc/Parowozy/Tkt48/Adhesion_Tkt48.inc")

Friction  (
		        1169N/m/s		-0.25		5.1mph	  15.771N/m/s	      1.530
		          5.1N/rad/s		1		-1rad/s		0		1
)
Inside (
PassengerCabinFile    ( PKP_TKt48-113.s  )
PassengerCabinHeadPos ( 1.75 3.3 -3.8 )
RotationLimit         ( 0 180 0 )
StartDirection        ( 0 0 0 )
Sound                 ( "..//..//common.snd//dampf_BR64//BR64Cab.sms" )
)

Include		("../common.inc/Parowozy/Tkt48/Lights_Tkt48_v2_m.inc")
)
Engine ( PKP_TKt48-113_m
Name ( "OR PKP TKt48-113 manewrowa MD Nysa//" )

Wagon ( PKP_TKt48-113_m )
Type                       ( Steam )
ORTSSteamLocomotiveType    ( Simple )


MaxTenderCoalMass    ( 6.0t )
MaxTenderWaterMass   ( 10.0t )

Include		("../common.inc/Parowozy/Tkt48/Parameters_Tkt48.inc")
Include ( "../common.inc/Parowozy/Tkt48/Settings_Tkt48.inc" )	
Include		("../common.inc/Parowozy/Tkt48/Effects_Tkt48.inc")
Include ( "../common.inc/Parowozy/Tkt48/Parameters_OR.inc" )
Include		("../common.inc/Parowozy/Tkt48/Compresor_Tkt48.inc")
Include		("../common.inc/Parowozy/Tkt48/Controling_Tkt48.inc")
        
Sound     ( "..//..//common.snd//dampf_BR64//BR64Cab.sms" )
CabView   ( "../../Common.cab/BR86/BR86.cvf" )
Include		("../common.inc/Parowozy/Tkt48/start_conf_Tkt48.inc")

Description ("Parowozy beztendrowe TKt48 /tetetka/ wykorzystywane były w 
lokalnym ruchu osobowym. 
Producent: Cegielski oraz Fablok. Lata 1950-1952
Producent: Fablok. Lata 1955-1957
Układ osi  1 – 4 – 1    
Masa służbowa:  98000 kg        
Prędkość maksymalna: 80kmh kmh   
Moc nominalna  785 kW     
Siła pociągowa 114kN  ")
)



