SIMISA@@@@@@@@@@JINX0h0t______

Tr_CabViewFile (
	CabViewType ( 2 )
	CabViewFile ( "..\\..\\common.cab\\BR285\\ER20front.ace" )
	Position ( 0.5 3.2 6 )
	Direction ( 14 -0.5 0 )
	
	CabViewFile ( "..\\..\\common.cab\\BR285\\ER20links.ace" )
	Position ( 0.5 3.2 6 )
	Direction ( 12 -34 0 )
	
	CabViewFile ( "..\\..\\common.cab\\BR285\\ER20rechts.ace" )
	Position ( 0 3.2 6 )
	Direction ( -5 86 0 )
	
	EngineData ( ER20_ALEX )
	
	CabViewControls ( 25
	
    DigitalClock (
      Type ( CLOCK DIGITAL_CLOCK )
      Position ( 270 330 0 0 )
	    Style ( 24HOUR )
      Accuracy ( 1 )
      ORTSFont ( 4 0 "Sans Serif" )
      ControlColour  ( 240 240 240 )
    )	
	  Digital (
		  Type ( TRACTION_BRAKING DIGITAL )
		  Position ( 270 317 0 0 )
		  ScaleRange ( 0 410 )
		  Accuracy ( 0 )
		  AccuracySwitch ( 0 )
		  LeadingZeros ( 0 )
		  Justification ( 1 )
		  PositiveColour ( 1
		  ControlColour ( 255 255 0  )
	  )
		  NegativeColour ( 0 )
	  	ORTSFont ( 4 1 "Sans Serif" )
		  DecreaseColour ( 0 )
		  Units ( KILO_NEWTONS )
    )
		Dial (
			Type ( BRAKE_CYL DIAL )
			Position ( 574 289 26 26 )
			Graphic ( "..\\..\\common.cab\\BR285\\ER20Nadel_rot.ace" )
			Style ( NEEDLE )
			ScaleRange ( 0 6 )
			ScalePos ( 235 150 )
			Units ( BAR )
			Pivot ( 18 )
			DirIncrease ( 0 )
		)
		Dial (
			Type ( ACCELEROMETER DIAL )
			Position ( 269 271 6 29 )
			Graphic ( "..\\..\\common.cab\\BR285\\ER20Nadel_schwarz.ace" )
			Style ( NEEDLE )
			ScaleRange ( -0.64 0.64 )
			ScalePos ( 225 135 )
                        Units ( KILO_NEWTONS )
			Pivot ( 27 )
			DirIncrease ( 0 )
		)
		Dial (
			Type ( SPEEDOMETER DIAL )
			Position ( 352 270 6 29 )
			Graphic ( "..\\..\\common.cab\\BR285\\ER20Nadel_schwarz.ace" )
			Style ( NEEDLE )
			ScaleRange ( 0 160 )
			ScalePos ( 225 135 )
			Units ( KM_PER_HOUR )
			Pivot ( 27 )
			DirIncrease ( 0 )
		)
		Dial (
			Type ( MAIN_RES DIAL )
			Position ( 569 341 23 23 )
			Graphic ( "..\\..\\common.cab\\BR285\\ER20Nadel_gelb.ace" )
			Style ( NEEDLE )
			ScaleRange ( 0 10 )
			ScalePos ( 235 130 )
			Units ( BAR )
			Pivot ( 16 )
			DirIncrease ( 0 )
		)
		Dial (
			Type ( BRAKE_PIPE DIAL )
			Position ( 567 339 26 26 )
			Graphic ( "..\\..\\common.cab\\BR285\\ER20Nadel_rot.ace" )
			Style ( NEEDLE )
			ScaleRange ( 0 10 )
			ScalePos ( 235 168 )
			Units ( BAR )
			Pivot ( 18 )
			DirIncrease ( 0 )
		)
		Lever (
			Type ( ENGINE_BRAKE LEVER )
			Position ( 586 323 60 120 )
			Graphic ( "..\\..\\common.cab\\BR285\\ER20Bremse2.ace" )
                        Style ( SPRUNG )
			MouseControl ( 1 )
			NumFrames ( 6 6 1 )
			NumPositions ( 6 3 2 1 0 4 5 )
			NumValues ( 3 0 0.1 0.2)
			Orientation ( 0 )
			DirIncrease ( 0 )
			ScaleRange ( 0 1 )
		)
		TriState (
			Type ( DIRECTION TRI_STATE )
			Position ( 102 390 25 22 )
			Graphic ( "..\\..\\common.cab\\BR285\\ER20Richt_Anz.ace" )
			NumFrames ( 3 3 1 )
			Style ( NONE )
			MouseControl ( 1 )
			Orientation ( 0 )
			DirIncrease ( 0 )
		)
		Lever (
			Type ( DYNAMIC_BRAKE LEVER )
			Position ( 569 436 15 15 )
			Graphic ( "..\\..\\common.cab\\BR285\\ER20Betr_Brems.ace" )
			Style ( SPRUNG )
			MouseControl ( 1 )
			NumFrames ( 2 2 1 )
			NumPositions ( 0 )
			NumValues ( 0 )
			Orientation ( 0 )
			DirIncrease ( 0 )
			ScaleRange ( 0 1 )
		)
		TriState (
			Type ( FRONT_HLIGHT TRI_STATE )
			Position ( 364 332 15 15 )
			Graphic ( "..\\..\\common.cab\\BR285\\ER20Licht.ace" )
			NumFrames ( 3 3 1 )
			Style ( NONE )
			MouseControl ( 1 )
			Orientation ( 0 )
			DirIncrease ( 0 )
		)
		TwoState (
			Type ( WIPERS TWO_STATE )
			Position ( 345 332 15 15 )
			Graphic ( "..\\..\\common.cab\\BR285\\ER20Start.ace" )
			NumFrames ( 2 2 1 )
			Style ( ONOFF )
			MouseControl ( 1 )
		)
		TwoState (
			Type ( HORN TWO_STATE )
			Position ( 578 464 19 16 )
			NumFrames ( 2 2 1 )
			Style ( WHILE_PRESSED )
			MouseControl ( 1 )
		)
     CombinedControl (
      Type ( CP_HANDLE COMBINED_CONTROL )
      Position ( 128 315 60 120 )
      Graphic ( "..\\..\\common.cab\\BR285\\ER20Fahrhebel.ace" )
      Style ( NONE )
      MouseControl ( 1 )
      NumFrames ( 6 6 1 )
      NumPositions ( 6 0 3 2 1 4 5 )
      NumValues ( 2 0 0.03)
      Orientation ( 0 )
      DirIncrease ( 0 )
    )
		Lever (
			Type ( TRAIN_BRAKE LEVER )
			Position ( 485 334 60 72 )
			Graphic ( "..\\..\\common.cab\\BR285\\ER20Bremse1.ace" )
			Style ( SPRUNG )
			MouseControl ( 1 )
			NumFrames ( 6 6 1 )
			NumPositions ( 6 0 1 2 3 4 5 )
			NumValues ( 0 )
			Orientation ( 0 )
			DirIncrease ( 0 )
			ScaleRange ( 0 1 )
		)
		TriState (
			Type ( DIRECTION TRI_STATE )
			Position ( 67 346 60 88 )
			Graphic ( "..\\..\\common.cab\\BR285\\ER20Wender.ace" )
			NumFrames ( 3 3 1 )
			Style ( NONE )
			MouseControl ( 1 )
			Orientation ( 0 )
			DirIncrease ( 0 )
		)
		MultiStateDisplay (
			Type ( FRICTION_BRAKING MULTI_STATE_DISPLAY )
			Position ( 250 331 18 18 )
			Graphic ( "..\\..\\common.cab\\BR285\\czuwak_lamp.ace" )
			States ( 2 2 1
				State (
					Style ( 0 )
					SwitchVal ( 0 )
				)
				State (
					Style ( 0 )
					SwitchVal ( 1 )
				)
			)
		)
			MultiStateDisplay (
			Type ( PENALTY_APP MULTI_STATE_DISPLAY )
			Position ( 250 331 16 16 )
			Graphic ( "..\\..\\common.cab\\BR285\\czuwak_lamp.ace" )
			States ( 2 2 1
				State (
					Style ( 0 )
					SwitchVal ( 0 )
				)
				State (
					Style ( 0 )
					SwitchVal ( 1 )
				)
			)
		)
		MultiStateDisplay (
			Type ( ALERTER_DISPLAY MULTI_STATE_DISPLAY )
			Position ( 364 343 17 17 )
			Graphic ( "..\\..\\common.cab\\BR285\\czuwak_lamp.ace" )
			States ( 2 2 1
				State (
					Style ( 0 )
					SwitchVal ( 0 )
				)
				State (
					Style ( 1 )
					SwitchVal ( 1 )
				)
			)
		)			
		TwoState (
			Type ( EMERGENCY_BRAKE TWO_STATE )
			Position ( 15 379 45 35 )
			Graphic ( "..\\..\\common.cab\\BR285\\ER20Notstop.ace" )
			NumFrames ( 2 2 1 )
			Style ( ONOFF )
			MouseControl ( 1 )
		)
	)
)